

ETKA

19:30

SG 45

Illustration 145-50

Restrictions UPD 133

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Model OCT | Year 2003 | MG  1 |  |  |  |  |  | 21.04.2022 |
|  | |

Remarks

KKK N 907 678 01 058 145 540

058 145 791

1AGU

M8X35 1

1

4X4

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Pos | Part Number | Name |  | Qty | Model |
| 1  (1)  (1)  (1)  (1)  2   3A   3B   4A   (5)   6  7  9   (9)  (9) | 06A 145 704 L  #06A 145 704 LX  >06A 145 713 D  #06A 145 713 DX  06A 145 713 F  06A 253 039 E   058 145 540   058 145 791   N 907 678 01   06A 145 536 B   N 010 247 10  N 103 036 03  06A 145 735 AA   06A 145 735 S  06A 145 735 AD | turbocharger  turbocharger   also use:  as required use:  turbocharger   also use:  as required use:  turbocharger  as required use:  F >> 1U-7A009 890\*  F >> 1U-78881 271\*  turbocharger  as required use:  F >> 1U-7A009 890\*  F >> 1U-78881 271\*  turbocharger  as required use:  F 1U-7A009 891>>\*  F 1U-78881 272>>\*  gasket  screw, hex. hd.  washer  stud  support part  bolt, hex. hd.,  self-locking  socket hd. screw with  collar  oil return line  oil return line  only for:  F >> 1U-7A009 890\*  F >> 1U-78881 271\*  oil return line   only for:  F 1U-7A009 891>>\*  F 1U-78881 272>>\* | 1.8ltr.  KKK N 907 678 01 058 145 540  058 145 791  KKK 06A 145 832 M 06A145867 E/M  KKK 06A 145 832 M 06A145867 E/M  KKK 06A 145 832 M 06A145867 E/M  M10X50  10,4X24X3  M10X35  M8X16  4X4 | 1  1  1  1  1  1  1  1  1  1  3  3  4  1  X  1  1 | AGU,AUM,ARX,  AUQ  AGU  AUQ,AUM,ARX  AUQ,AUM,ARX  AUQ,AUM,ARX |

Illustration

Restrictions UPD 133

Remarks

A12X15,5X1,5 X

M6X22SPZ1 X

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
| 10  (10)  11  13   14   16  (16)  17A  (17A)  24   25  30A  31  (31)  32 | 058 145 757 B  058 145 757 C  N 014 702 10  06A 145 541 H   N 013 814 9   N 013 812 8  N 013 851 4  06A 145 778 D  06A 145 778 Q  058 145 757 A   N 100 863 02  06A 121 497 Q  N 021 074 2  06A 145 541 J  N 013 814 9 | gasket  F >> 1U-4-830 086\*  F >> 1U-48720 053\*  gasket  F 1U-4-830 087>>\*  F 1U-48720 054>>\*  bolt, with hex. socket  hd.  banjo bolt  sealing washer  sealing washer  F >> 1U-3-704 906  F >> 1U-3A006 980  F >> 1U-38677 465  sealing washer  F 1U-3-704 907>>  F 1U-3A006 981>>  F 1U-38677 466>>  oil pipe  F >> 1U-3-704 906  F >> 1U-3A006 980  F >> 1U-38677 465  oil pipe  F 1U-3-704 907>>  F 1U-3A006 981>>  F 1U-38677 466>>  gasket  bolt, with hex. socket hd.  (combi.)  water hose  (adapters >  turbocharger)   also use:  banjo bolt  F >> 1U-3-696 896  F >> 1U-3A006 571  F >> 1U-38675 072  banjo bolt  F 1U-3-696 897>>  F 1U-3A006 572>>  F 1U-38675 073>>  sealing washer  F >> 1U-3-696 896  F >> 1U-3A006 571  F >> 1U-38675 072 | M6X15  M14X1,5X38  14X18X1,5  A12X18  feed  N 013 849 5 06A 145 541 J  10  10  14X18X1,5 | 1  1  X  1  1  1  1  1  1  1  2  2  2 |  |

Remarks

1

1

1

(38) 8L0 145 718 C pressure controlline

as required use: 06A 145 712 C

028 103 657

N 020 902 2

LL8 1

\*

\*

\*

- 06A 121 279 spacer 1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Pos | Part Number | Name |  | Qty | Model |
| (32)  35   36   38  39   40   41  (41)  (41)  42  42A  (42A) | N 013 849 5  N 102 582 01   058 906 283 F   06A 145 712 C  N 024 528 1   N 012 226 5   N 021 071 5  06A 145 541 A  WHT 000 223  06A 121 492 AB  06A 121 492 AD  06A 121 492 AG | sealing washer  F 1U-3-696 897>>  F 1U-3A006 572>>  F 1U-38675 073>>  clamp  solenoid valve  pressure controlline  as required use:  clamp  spring washer  banjo bolt  F >> 1U-6A036 517\*  F >> 1U-68863 540\*  banjo bolt  (for turbocharger)  F >> 1U-6A036 517\*  F >> 1U-68863 540\*  banjo bolt  F 1U-6A036 518>>\*  F 1U-68863 541>>\*  water pipe  F >> 1U-4-898 054\*  F >> 1U-4A019 552\*  F >> 1U-48745 256\*  water pipe  F 1U-4-898 055>>  F 1U-4A019 553>> 1U-7A009 890\*  F 1U-48745 257>> 1U-78881 271\*   as required use:  water pipe  F 1U-7A009 891>>\*  F 1U-78881 272>>\*  as required use: | A14X20  AL12-22  8L0 145 718 C  028 145 657  N 020 902 2  LC8-12  B6X12X0,5  LL8  return  (KOMPLET)  06A 145 541 H  06A 121 279  N 013 814 9  06A 145 541 H  06A 121 279  N 013 814 9 | 2  X  1  1  1  1  X  1  1  1  1  1  \*  \*  \*  1 |  |