

ETKA

19:30

SG 45

Illustration 145-50

Restrictions UPD 133

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Model OCT  | Year 2003  | MG 1  |  |  |  |  |  | 21.04.2022  |
|  |

Remarks

 KKK N 907 678 01 058 145 540

058 145 791

1AGU

M8X35 1

1

4X4

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Pos  | Part Number  | Name  |  | Qty  | Model  |
|  1  (1)  (1)  (1)  (1)  2  3A  3B  4A  (5)  6  7  9  (9)  (9)  |  06A 145 704 L  #06A 145 704 LX  >06A 145 713 D  #06A 145 713 DX  06A 145 713 F  06A 253 039 E  058 145 540  058 145 791  N 907 678 01  06A 145 536 B  N 010 247 10  N 103 036 03  06A 145 735 AA  06A 145 735 S  06A 145 735 AD  | turbocharger turbocharger  also use:  as required use: turbocharger  also use:  as required use: turbocharger  as required use: F >> 1U-7A009 890\* F >> 1U-78881 271\* turbocharger  as required use: F >> 1U-7A009 890\* F >> 1U-78881 271\* turbocharger  as required use: F 1U-7A009 891>>\* F 1U-78881 272>>\* gasket screw, hex. hd. washer stud support part bolt, hex. hd., self-locking socket hd. screw with collar oil return line oil return line  only for: F >> 1U-7A009 890\* F >> 1U-78881 271\* oil return line  only for: F 1U-7A009 891>>\* F 1U-78881 272>>\*  | 1.8ltr.  KKK N 907 678 01 058 145 540 058 145 791  KKK 06A 145 832 M 06A145867 E/M  KKK 06A 145 832 M 06A145867 E/M  KKK 06A 145 832 M 06A145867 E/M M10X50 10,4X24X3 M10X35 M8X16 4X4  | 1 1 1 1 1 1 1 1 1 1 3 3 4 1 X 1 1  | AGU,AUM,ARX, AUQ AGU AUQ,AUM,ARX AUQ,AUM,ARX AUQ,AUM,ARX  |

Illustration

Restrictions UPD 133

Remarks

A12X15,5X1,5 X

M6X22SPZ1 X

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
|  10  (10)  11  13  14  16  (16)  17A (17A)  24  25  30A  31  (31)  32  |  058 145 757 B  058 145 757 C  N 014 702 10  06A 145 541 H  N 013 814 9  N 013 812 8  N 013 851 4  06A 145 778 D  06A 145 778 Q  058 145 757 A  N 100 863 02  06A 121 497 Q  N 021 074 2  06A 145 541 J  N 013 814 9  | gasket F >> 1U-4-830 086\* F >> 1U-48720 053\* gasket F 1U-4-830 087>>\* F 1U-48720 054>>\* bolt, with hex. socket hd. banjo bolt sealing washer sealing washer F >> 1U-3-704 906 F >> 1U-3A006 980 F >> 1U-38677 465 sealing washer F 1U-3-704 907>> F 1U-3A006 981>> F 1U-38677 466>> oil pipe F >> 1U-3-704 906 F >> 1U-3A006 980 F >> 1U-38677 465 oil pipe F 1U-3-704 907>> F 1U-3A006 981>> F 1U-38677 466>> gasket bolt, with hex. socket hd. (combi.) water hose (adapters >  turbocharger)  also use: banjo bolt F >> 1U-3-696 896 F >> 1U-3A006 571 F >> 1U-38675 072 banjo bolt F 1U-3-696 897>> F 1U-3A006 572>> F 1U-38675 073>> sealing washer F >> 1U-3-696 896 F >> 1U-3A006 571 F >> 1U-38675 072  | M6X15 M14X1,5X38 14X18X1,5 A12X18 feed N 013 849 5 06A 145 541 J 10 10 14X18X1,5  | 1 1 X 1 1 1 1 1 1 1 2 2 2  |  |

Remarks

1

1

1

 (38) 8L0 145 718 C pressure controlline

 as required use: 06A 145 712 C

028 103 657

N 020 902 2

LL8 1

\*

\*

\*

 - 06A 121 279 spacer 1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Pos  | Part Number  | Name  |  | Qty  | Model  |
|  (32)  35  36  38  39  40  41  (41)  (41)  42  42A (42A)  |  N 013 849 5  N 102 582 01  058 906 283 F  06A 145 712 C  N 024 528 1  N 012 226 5  N 021 071 5  06A 145 541 A  WHT 000 223  06A 121 492 AB  06A 121 492 AD  06A 121 492 AG  | sealing washer F 1U-3-696 897>> F 1U-3A006 572>> F 1U-38675 073>> clamp solenoid valve pressure controlline  as required use: clamp spring washer banjo bolt F >> 1U-6A036 517\* F >> 1U-68863 540\* banjo bolt (for turbocharger) F >> 1U-6A036 517\* F >> 1U-68863 540\* banjo bolt F 1U-6A036 518>>\* F 1U-68863 541>>\* water pipe F >> 1U-4-898 054\* F >> 1U-4A019 552\* F >> 1U-48745 256\* water pipe F 1U-4-898 055>> F 1U-4A019 553>> 1U-7A009 890\* F 1U-48745 257>> 1U-78881 271\*  as required use: water pipe F 1U-7A009 891>>\* F 1U-78881 272>>\*  as required use:  | A14X20 AL12-22 8L0 145 718 C 028 145 657 N 020 902 2 LC8-12 B6X12X0,5 LL8 return (KOMPLET) 06A 145 541 H 06A 121 279 N 013 814 9 06A 145 541 H 06A 121 279 N 013 814 9  | 2 X 1 1 1 1 X 1 1 1 1 1 \* \* \* 1  |  |